,Wattage Comments##OTHER##,Wattage##ELECTRICAL_WATTAGE##WATTS,Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS,Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT,Initial Color Temperature##COLOR_TEMPERATURE##KELVIN,Tilt Angle##OTHER##,IES Files Link##OTHER##,Photometric Web File##OTHER##,URL##OTHER##,Type Comments##OTHER##,Model##OTHER##,Manufacturer##OTHER##,Description##OTHER##
BOLD-3-HL-WW-IC-1200L-40K-90-DIM10-MVOLT-B3R-307-A-F-CL-WH,13W,13.0,1135.0,87,4000,-90,https://epl.com/media/ies/bold-3-hl-ww-ic.zip,BOLD-3-HL-WW-IC-1200L-40K-90-DIM10-MVOLT-B3R-307-A-F-CL-WH.ies,https://epl.com/product/bold-3-hl-ww-ic/,Bold,BOLD-3-HL-WW-IC,Edison Price Lighting,3 Inch Round High-Lumen Wallwash IC-Rated Downlight
BOLD-3-HL-WW-IC-1500L-40K-90-DIM10-MVOLT-B3R-307-A-F-CL-WH,17W,17.0,1418.0,83,4000,-90,https://epl.com/media/ies/bold-3-hl-ww-ic.zip,BOLD-3-HL-WW-IC-1500L-40K-90-DIM10-MVOLT-B3R-307-A-F-CL-WH.ies,https://epl.com/product/bold-3-hl-ww-ic/,Bold,BOLD-3-HL-WW-IC,Edison Price Lighting,3 Inch Round High-Lumen Wallwash IC-Rated Downlight
BOLD-3-HL-WW-IC-2000L-40K-90-DIM10-MVOLT-B3R-307-A-F-CL-WH,22W,22.2,1891.0,85,4000,-90,https://epl.com/media/ies/bold-3-hl-ww-ic.zip,BOLD-3-HL-WW-IC-2000L-40K-90-DIM10-MVOLT-B3R-307-A-F-CL-WH.ies,https://epl.com/product/bold-3-hl-ww-ic/,Bold,BOLD-3-HL-WW-IC,Edison Price Lighting,3 Inch Round High-Lumen Wallwash IC-Rated Downlight
BOLD-3-HL-WW-IC-900L-40K-90-DIM10-MVOLT-B3R-307-A-F-CL-WH,10W,10.3,851.0,83,4000,-90,https://epl.com/media/ies/bold-3-hl-ww-ic.zip,BOLD-3-HL-WW-IC-900L-40K-90-DIM10-MVOLT-B3R-307-A-F-CL-WH.ies,https://epl.com/product/bold-3-hl-ww-ic/,Bold,BOLD-3-HL-WW-IC,Edison Price Lighting,3 Inch Round High-Lumen Wallwash IC-Rated Downlight
